20XX-01-XXXX

Road Curvature Decomposition for Autonomous Guidance

Author, co-author (Do NOT enter this information. It will be pulled from participant tab in MyTechZone)

Affiliation (Do NOT enter this information. It will be pulled from participant tab in MyTechZone)

Abstract

Vehicle autonomy is critically dependent on an accurate identification and mathematical representation of road and lane geometries. Many road lane identification systems are ad hoc (e.g., machine vision and lane keeping systems) or rely on polynomial approximations of road data and GPS positioning. A novel system is proposed in which geodetic road data is parsed along road directions and digitally stored in a road data matrix. Using mapping algorithms, the road data is converted to a smooth, differentiable path which connects critical road coordinates with curvature vectors and changes to road tangent angles. Different road data sources such as GPS or geographical scans were evaluated with this method and compared to current road design standards as per the American Association of State Highway and Transportation Officials. This approach takes advantage of standard roadway design practices, which rely on speed limit, superelevation, and empirical data for maximum lateral acceleration tolerance to determine acceptable radii of curvature for different classes of roadways. Successful implementation of this technology could accelerate autonomous vehicle’s navigation research and development for new guidance paradigms in addition to traditional machine vision-based systems.

Keywords: Trajectory Generation, Path Generation, Curvature, AASHTO, V2I, Vehicle-to-Infrastructure

Introduction

Road geometries play a circumstantial role in designing for transportation. In autonomous vehicles, the current level of vehicle autonomy depends heavily on light sensors or radar sensor for detecting both objects and lane markings on the road. Based on this sensor information, vehicles can generate paths and trajectory approximations of where the vehicle should be going. In motion planning, a path is defined a set of possible ways a vehicle can go from Point A to Point B. While trajectory is defined as the profile needed to go through that path given different constraints. For example, many trajectories can lie inside of a given path as shown in Figure 1. Given constraints can be in the form of differential constraints from equations of motion, geometrical constraints or dynamic constraints from vehicle limits.



Figure . Different Trajectories in a Given Path from Point A to Point B.

From literature, local trajectory generation techniques utilize different mathematical models. Such methods can be classified as roadmap-based planning [Heinrich, S.,], sampling-based planning [Heinrich, S.,], probabilistic methods [Heinrich, S.,], and variational methods [Fox, Charles,]. Most of these methods rely with the aid of vehicle sensors to generate their navigation map, for example discretizing areas of space from an image and classifying them as either navigation feasible or not. However, variational methods can be exploited outside of its dependence on image processing.

Variational methods arise from optimizing functionals with non-holonomic constraints (i.e. constraints on the velocity and acceleration). The methods yield polynomial solutions of high order that are treated as boundary value problems (BVP) during vehicle navigation [Takahshi, A.,]. Along with variational methods, Clothoid functions (Cornu Spirals or Euler Spiral) are often studied in autonomous research because of their effectiveness to connect a straight line with a constant radius curve. Such that clothoids are used for road design and local trajectory generations [Thrun].

These trajectory methods are then combined with optimization theory to be implemented into controllers for navigation purposes [Thrun]. In general, these trajectories focus on providing a continuous function (up to the third derivative) while being smooth (i.e. minimizing the jerk ). However, trajectories can also be generated from offline information that comes from different media such as GPS or geospatial data. Therefore, offline data provides a static calculation of the trajectories a vehicle should have regardless of any sensor error that vehicles could encounter during their trajectory calculations.

Thus, the objective of this research study is to develop a deterministic technique for identifying the centerline path of travel lanes using smooth, differentiable, parametric equations and geospatial road data. The rest of this paper is composed of the following sections: Method Formulation, Implementations, Recommendations and Conclusions.

Method Formulation

1.1 Reference Configuration

The method presented formulates a point particle dynamics approach describing the vehicle’s motion as it passes through a road. A Frenet-Serret reference frame is used along with unit vectors of N (normal), T (tangential), and B (binormal, out of plane) as shown in Figure 2. For this paper, it is assumed that the vehicle navigates on a 2D Euclidean Space.



Figure . Normal-Tangential Coordinates Example in Vehicle’s Center of Mass.

As the vehicle goes through the curve, it is limited to constraints provided by road geometry and friction limits on the vehicle tires [Pacejka] [Gillespie]. These limits are related to the acceleration a vehicle goes under circular motion, which is denoted as:

Where:

a = Total Acceleration of Vehicle (m/s2)

v = Tangential Velocity of Vehicle (m/s)

= Curvature at an Instantaneous Point (m-1)

N =Normal Unit Vector

T= Tangential Unit Vector

Curvature can be defined analytically, physically and geometrically. It measures how fast the tangential unit vector T changes with respect to an instantaneous point in the curve. Many researchers have been developed on basis of curvature formulation [Do Carmo][O Reilly][Add More]. By Frenet-Serret definition of coordinates, curvature can be expressed in a vector form that has a direction parallel to the Normal Unit Vector shown in Figure 2. Similarly, a vector perpendicular to the curvature direction will provide a velocity tangent vector approximation at that point. This velocity vector provides a heading angle to the desired trajectory that is needed to follow a road path. Thus, it is possible to obtain a heading angle representation of any trajectory if curvatures can be obtained from a discrete data set.

1.2 Discrete Curvature Formulation

To obtain the curvature, let a scalene triangle with corners A, B, C have a circumscribed circle of radius R in Euclidean 2D space as shown in Figure 3.



Figure . Circumscribed Circle in Scalene Triangle.

If we let a vector D be the cross product in between the vectors AB and AC, the direction will be pointing out normal to the plane defined by the intersection of AB and AC. By definition of the magnitude for cross product:

Let a vector E be the cross product of D with the vector AB, defining this new vector in the direction of as shown in red in Figure 4. Let the magnitude of vector E be defined as:



Figure . First Unit Vector Direction on Triangle.

Similarly, let a vector F be the cross product of D with the vector AC, defining this new vector in the direction of shown in blue in Figure 5. Let the magnitude of vector E be defined as:



Figure . First- and Second-Unit Vectors on Triangle.

The unit vectors of and are defined by the following:

By definition, the midsection of any triangle’s side intersects with each other at a point P as shown in Figure 6. These intersecting lines denote two triangles with the same angle in between the unit vectors and their corresponding midsections as shown below.



Figure . Radius of Curvature obtained from Geometric Relationships.

From these triangles, it is possible to break the vector DP into components along unit vectors and to obtain a new definition of DP in a different set of coordinates as follows:

From our previous definition of the vector D, it is possible to simplify further:

With these components, it is possible to obtain the magnitude as follows:

Using previous definitions of E and F:

Using previous definition of D, it is possible to obtain the radius of the prescribed circle in terms of only the difference in between points A, B and C.

Using the previous definition, it is possible to apply the formulation of R to differentially smaller arc segments as it is shown in Figure 7 below.



Figure . Scalene Triangle in Small Arc-Segment.

The radius of this circumscribed circle is called radius of curvature, and its inverse is known as curvature denoted as the formula below [?].

Through this definition, it is possible to extend the application of this discrete radius of curvature and applying it to long-discrete arc segments as shown in Figure 8.



Figure . Road Section with Discrete Sections

1.3 Heading Angle Calculations

By sampling at a rate of three location points per curvature point, it is possible to create a discrete representation of the road with curvature data. To obtain the heading angle, two options were used. The first one comes from the well-established definition of heading angle from trigonometric relationships. The arc-length s of a curve is defined as the length traveled by a certain amount of degrees along a constant radius r. If s is sufficiently small, a triangle can be formed in between these three parameters, which are related through geometry:

Defining r as the radius of curvature at the specific arc-length and letting.

By the previous assumption of small angles: , which leads to:

Let the Curvature be denoted by (#), and substituting this definition into equation (1)

Assuming a differential section for and. Rearranging for:

By separation of variables and integration

Which concludes that the angle of orientation as a function of arc-length s can be found through numerical integration of the curvature as:

The second one involves an orthogonal phase shift to the curvature direction. Which by definition of the Frenet-Serret, can be obtained from the components of the curvature previously calculated in Equation (#). Using the discrete curvature formulation, the two heading angle calculations were implemented in the next section.

Implementations

Typical highway roads are designed based on AASHTO guidelines to provide a natural, easy-to-follow path for drivers, such that the lateral force increases and decreases gradually as the vehicle enters and leaves a circular curve [AASHTO]. This leads the advantage of generating curves based on AASHTO road geometry to obtain heading angles. The radius of curvature is computed from discrete points that represent coordinates of a road. To obtain different approximations, different methods to coordinates were used. The first method involved a base model of the road based on AASHTO guidelines, and the second method involved using Google Earth coordinates.

2.1 AASHTO Base Model

This model consisted on strictly using AASHTO guidelines to design an ideal highway road for a vehicle traversing at constant 60 mph. The curve consisted of 5 different sections that can be classified as: straight section, entrance transition, constant radius curve, exit transition and straight section. Applying the discrete geometric approach to this curve, curvature vectors were plotted with respect to the road segments as shown Figure 9. The curvature magnitude was plotted with respect to road segments to obtain a base curvature profile as shown in Figure 10.



Figure . AASHTO Base Model: Road with Curvature Vectors.



Figure . AASHTO Base Model: Curvature κ vs. Cumulative Curve Length.

With the curvature profile established, two different approaches were used to confirm the heading angle approximation. One method involved obtaining the heading angle from trigonometric functions on the curvature vectors and add an orthogonal phase shift. The second method involved numerical integration of the curvature data to obtain a heading angle. The proof of the method is shown in [Appendix] and both methods are shown in Figure 11 and Figure 12. Results on heading angles with respect to road segments are shown in Figure 13. These resulting angles were used as input data on a controller developed in [Michael].



Figure . AASHTO Base Model: Orthogonal Phase Shift Approach.



Figure . AASHTO Base Model: Numerical Integration Approach.



Figure . AASHTO Base Model: Road with Velocity Vectors.

2.2 Google Earth Model

This model is based off a selection of points in Google Earth that represent a highway road with design speed of 60 mph. The points were picked as close as possible to resemble the road centerline of the highway. The road profile and resulting vectors from applying the discrete geometry approach are shown in Figure 14. It is noticeable how the vector directions choose arbitrary tangent directions when the curve approaches a straight-line section. The curvature magnitude with respect to length was also plotted in Figure 15 and it was observed that magnitude deviations increased considerably compared to the ideal AASHTO model.



Figure . Google Earth Model: Road with Velocity Vectors.



Figure . Google Earth Model: Curvature κ vs. Cumulative Curve Length.

The method was not efficient in calculating curvature magnitudes, but the direction of the heading angle obtained from the orthogonal phase shift still provided comparable results to those found by calculating with AASHTO as shown in Figure 16. Similarly, the resulting velocity vectors to guide the vehicle provide a suitable heading direction as shown in Figure 17. These resulting angles were used as input data on a controller developed in [Michael] to study the efficiency of navigating with this input information.



Figure . Google Earth Model: Orthogonal Phase Shift Approach.



Figure . Google Earth Model: Road with Velocity Vectors.

*2.3 Global Positioning System Model*

The last model is based off a GPS data set collected from a road with speed limit of 60 mph. The data was collected with a VC4000 Unit at a frequency rate of ## Hz.

Discussion/Recommendations

The study presented has the potential to be implemented on different areas in which path navigation is utilized. Such as unmanned aerial systems, or mobile robots. For this project, the route of autonomous vehicles is chosen to be the implementation of this technique. The advantages of this backup system rely on offering a backup system to the light and radar sensors on a vehicle. For example, on snow/rain conditions, the projected navigation path can provide a weighting factor on decision making for a given autonomous vehicle. To achieve this goal, the following scheme is proposed for an implementation of the discrete road decomposition. The first step involves collection of road data through any convenient means: GPS Data, Surveying, Aerial Scanning. This road data contains a representation of the road centerlines which can be exported in different formats. These road centerlines are decomposed with the proposed method and then stored in a local infrastructure station. This infrastructure localizes and transmits the heading instructions for any upcoming vehicle through the designated road. Finally, a controller is developed to consider the heading based from the discrete road decomposition and navigate safely through the road.

Summary/Conclusions

In conclusion, a novel method was proposed to calculate trajectories based on road data. Furthermore, the method exploits the perpendicular relationship in between the safe curvature design of any AASHTO designed road along with the heading angle of a vehicle. The method will be further explored with a refined/different data sets from other sources and testing for the feasibility of navigation. Successful implementation of this method could offer a new key piece to solve the autonomous vehicle paradigm under weather disruptions and/or other navigation technologies.

References

1. Werling, M., Ziegler, J., Soren, K., and Thrun, S., “Optimal Trajectory Generation for Dynamic Street Scenarios in a Frenet Frame,” 2010
2. Kelly, A., Nagy B., “Reactive Nonholonomic Trajectory Generation via Parametric Optimal Control,” 2003
3. Sun, Y., Zhan, Z., Fang, Y., Zheng, L. et al., “A Dynamic Local Trajectory Planning and Tracking Method for UGV Based on Optimal Algorithm,” 2019
4. Takahashi, A., Hongo, T., Ninomiya, Y., and Sugimoto, G., “Local Path Planning and Motion Control for AGV in Positioning,” 1989
5. Piazzi, A. and Guarino lo Bianco, C., “Quintic G2-Splines for Trajectory Planning of Autonomous Vehicles,” 2000
6. Wilde, D., “Computing Clothoid-Arc Segments for Trajectory Generation,” 2009
7. Delingette, H., Hebert, M., Ikeuchi, K., “Trajectory Generation with Curvature Constraint based on Energy Minimization,” 1991
8. Van Vliet, L. J., Verbeek, P. W., “Curvature and Bending Energy in Digitized 2D and 3D Images,” 1993
9. Guillaume, P., Schoukens J., Pintelon, R., “Sensitivity of Roots to Errors in the Coefficient of Polynomials Obtained by Frequency –Domain Estimation Methods,” 1989
10. Atkinson, K. E., “An Introduction to Numerical Analysis,” 1989
11. O’Reilly, O. M., “Engineering Dynamics A Primer,” 2010
12. Pressley, A. N. “Elementary Differential Geometry,” 2010
13. Pacejka, H. B. “Tyre and Vehicle Dynamics,” 2006
14. Gillespie, T. D. “Fundamentals of Vehicle Dynamics,” 1992
15. Do Carmo, M. P., “Differential Geometry of Curves and Surfaces,” 1976
16. AASHTO, A Policy on Geometric Design of Highways and Streets, 2011
17. Mjaavatten, A. “Curvature of a Discrete Curve in 3D Space,” 2018
18. Duhn, M., Parikh, G., Hourdos, J., “I-94 Connected Vehicles Testbed Operations and Maintenance,” 2019
19. Druta, A. S. Alden, Implementation and Evaluation of a Buried Cable Animal Detection System and Deer Warning Sign, 2019
20. SAE International, J3016-Taxonomy and Definitions for Terms Related to Driving Automation Systems for On-Road Motor Vehicles, 2018
21. William J. Hughes Technical Center, Global Positioning System (GPS) Standard Positioning Service (SPS) Performance Analysis Report, 2017
22. Heinrich, S., “Planning Universal On-Road Driving Strategies for Automated Vehicles,” 2018

Contact Information

Contact details for the main author should be included here. Details may include mailing address, email address, and/or telephone number (whichever is deemed appropriate).

Acknowledgments

If the Acknowledgments section is not wanted, delete this heading and text.

Appendix

A.1 - *Heading Angle Trigonometric Formulation*

The arc-length s of a curve is defined as the length traveled by a certain amount of degrees along a constant radius r. If s is sufficiently small, a triangle can be formed in between these three parameters, which are related through geometry:

Defining r as the radius of curvature at the specific arc-length and letting.

By the previous assumption of small angles:

Which leads to

(1)

Let the Curvature be denoted as

Substituting this definition into equation (1)

Assuming a differential section for and. Rearranging for:

By separation of variables and integration

Which concludes that the angle of orientation as a function of arc-length s can be found through numerical integration of the curvature as: