**Trajectory Generation Background**

In motion planning, a path is defined a set of possible ways a vehicle is allowed to go from Point A to Point B. While trajectory is defined as the profile needed to go through that path given different constraints. For example, many trajectories can lie inside of a given path as shown in Figure 1. Given constraints can be in the form of differential constraints from equations of motion, geometrical constraints or dynamic constraints from vehicle limits.

